100, Error Inserting PROM change flag : 
101, Unable to Read PROM : timed out
102, Error
103, Error Reading PROM/Memory function : 
104, Programming
105, PROM PROGRAMMING IN PROGRESS
106, Error Writing PROM Data : 
107, Error Decoding PROM Data : 
108,      Thickness Diameter  Material
109,      Thickness Diameter  Material
110, Coin --------- --------- ---------
111, Coin --------- --------- ---------
112, Values  A   B   C   D   E   F
113, Values  A   B   C   D   E   F
114, Error Displaying PROM Data : 
115, Error Mapping PROM Data : 
116, Error Mapping CC Routing Data : 
117, PROM COPY SOURCE ERROR ME181
118, Error Copying Old PROM Data : 
119, Error Calculating Normal Distribution : 
120, Error in Normal Lookup Table : 
121, Error Setting Up Validator Test Form : 
122, No Response from Programmer Box
123, Comms Error
124, Validator NOT DETECTED
125, Validator Check
126, Error Checking Validator Connected : 
127, EEPROM Read
128, READING EEPROM IN PROGRESS
129, Incompatible CC Interface Board
130, Error Reading EEPROM Address : 
131, NRI Memory Read
132, READING MEMORY IN PROGRESS
133, No Communication with the NRI Coin Mech
134,  or Wrong Mech Type
135, Check Coin Mech Type and Connections
136, Error Reading NRI Memory Address : 
137, NRI Memory 
138, PROGRAMMING MEMORY IN PROGRESS
139, No Communication with the NRI Coin Mech
140,  or Wrong Mech Type
141, Check Coin Mech Type and Connections
142, Error Programming NRI Memory
143, NRI Memory Programmed OK
144, OK
145, Error NRI Memory Programming routine : 
146, Timeout reading Coin Mech EEPROM
147, Timeout reading Coin Mech EEPROM
148, Checksum Error reading Coin Mech EEPROM Address:
149, Error Reading EEPROM Address : 
150, Error Writing EEPROM Address : 
151, 3*SD
152, 2*SD
153, Mean
154, Low
155, High
156, Fixed
157, Error Mapping C120 Outputs : 
200, Error Adding Coinset References to PROM : 
201, Put a floppy disk in the drive and close the door.
202, This drive or path does not exist: 
203, Unexpected error #
204,  occurred: 
205, Error Mapping Data to ME181 PROM : 
206, Error Sending Data : 
207, Error Sending Data 2 : 
208, Error detected
209, Error loading Mech Type List : 
210, Error Clearing Validator Test form : 
211, Insert PROM to check. Switch 1 ON, Switch 2 OFF on Mektek E+1 device
212, Load PROM
213, Verify PROM OK
214, Verify
215, Verify PROM FAILED
216, Error in PROM Verify routine : 
217, Error Mapping Checked PROM Segments : 
218, Failed to set up validator timings after 5 retries
219, Error
220, Error setting up Coin Mech Timings : 
221, Error Checking Mech Type is valid : 
222, Insufficient credits available
223, Available: 
224,   Required: 
225, Deduct Credits
226, Deducting 
227,  credits
228, Deduct Credits
229, Credits are low - Order more?
230, Credits
231, Parameter
232, Thickness
233, Diameter
234, Material
235, NFP
236, GRO
237, NFA
238, HFP
240, NFP
241, GRO
242, GRU
243, NFA
244, RCH
245, HFP
246, MNF
247, GRO
248, GRU
249, MHF
250, NFP
251, GRO
252, GRU
253, NFA
254, RCH
255, HFP
300, Serial Mode Not Set-up
301, Error
302, Stuck in Serial Comms Mode
303, Error Reading EEPROM Address : 
304, Error parsing CC parameters : 
305, EEPROM Programming
306, WRITING EEPROM IN PROGRESS
307, error writing EEPROM address :
308, Error
309, error writing EEPROM address :
310, Error
311, Error Writing EEPROM : 
312, Error Enabling Coin Data : 
313, Error decoding G13 parameter string : 
314, Error getting CC coin data : 
315, Error getting NRI parameter values : 
316,    EEPROM Verified OK   
317, EEPROM VERIFY
318,    EEPROM Verify FAIL   
319, EEPROM VERIFY
320, G18 requires Resistor Link Modification
321, or Alternative Interface Board
322, G18 Warning
323, Error decoding G13 parameter string : 
324, Error mapping old NRI parameters : 
325, Hardware error : I2C Clock and Data lines stuck
326, Error
327, Error setting up I2C mode : 
328, Error ending I2C mode : 
329, Error getting I2C data : 
330, No ACK reading Coin Mech EEPROM
331, Error
332, Error Reading Sentinel EEPROM Address : 
333, Error Writing Sentinel EEPROM Address : 
400, Error Updating Checked PROM Segments : 
401, Error Unloading Coin Measure form : 
402, Error Updating latest results : 
403, Error Calculating Stats : 
404, Error Cancelling Wizard routine : 
405, Invalid Filename
406, Error
407, Cancel Operation
408, Invalid Coin Mech Type: 
409, Warning
410, Invalid Coin Mech Manufacturer: 
411, Back to Main Window
412, Error: Sensor Idle readings out of Limits
413, Idles:       
414, Readings:    
415, Limits: 
416, Cause:  Incorrect mech type selected or faulty validator
417, Error
418, Data Gathering Complete
419, Complete
420, Insert Old PROM to COPY
421, Mektek E+1 : Switch 1 ON and Switch 2 OFF
422, Copy PROM
423, Remove OLD PROM from Socket
424, Error Transferring PROM data : 
425, PROM Segment
426, Coin Channel
427, Coin Channel
428, Output Line
429, Error in Wizard routine : 
430, Error Loading Coin Measurement form : 
431, Error Updating Results Display : 
432, Error Calculating target coin number : 
433, Slug 3SD Limits
434, Slug Separation
435, Error Showing Slug display format : 
436, PROM Limits
437, Limit Source
438, Error Showing Coin display format : 
439, Error handling 1K option in Coin Measure form : 
440, Error handling 2K option in Coin Measure form : 
441, Error Building Target Coin list : 
442, Error Adding Coin to Target list : 
443, Error Building Segment list : 
444, Capture Measurements : 
445, Back to Main Window
446, Number of Coins Remaining
447, Error Initialising Coin Measure Form : 
448, Overwrite Existing File
449, Warning
450, Error Clearing Initial Prom Data : 
451, Too Many Slug Records
452, Coinset Error
453, Too Many Coins to One Channel
454, Coinset Error
455, Error Parsing Data Records for transfer : 
456, Pass 1 Eliminating (
457, ) - on parameter
458,  Reading 
459,  Means 
460, Pass 2 Eliminating (
461, ) - on parameter
462,  Reading 
463,  Means 
464,  Coin Fliers detected
465, Need to redrop 
466,  Coins
467, Press OK to accept Elimination of Fliers
468, Press CANCEL to Skip Elimination
469, Data Error
470, Error in Flier Elimination Routine : 
471, Wizard
472, Cancel Operation
473, Invalid Coin Value has been Set
474, Must be a multiple of: 
475, Error
476, Invalid Coin Value has been Set
477, Must be a multiple of: 
478, Error
479, 2*SD
480, Low
481, Fixed
482, High
483, Fixed
484, Coin to Add or Replace
485, Coin to Measure
486, Start Coin Drop
487, Gathered Coin Data
488, Slug to Fix
489, Start Slug Drop
490, Gathered Slug Data
491, Start Coin Type: 
492, CANCEL to SKIP Coin
493, Data Gather
494, Gathered Coin 
495, Error Gathering Coin Drop data : 
510, Coinset Description
511, Ref. Code
512, Ver.
513, Coin Channel
514, Coin Description
515, Mech. Type
516, Number of Coins Remaining
517, Measurements
518, Parameter 1
519, Parameter 2
520, Parameter 3
521, Parameter 4
522, Parameter 5
523, Parameter 6
524, Measurement
525, Mean
526, SD
527, Lowest/Highest
528, Limit Source
529, Offset
530, PROM Limits
531, Log Results
532, PROM size
533, PROM Segments
534, Run Coinset File
535, Wizards
536, Cancel Operation
537, Coin Wizards
538, Mech Type
539, PROM Segments
540, Coin Channel
541, Coin Value
542, Inhibit Line
543, Add/Replace Coin
544, Wizards
545, Cancel Operation
546, Edit Limits
547, Slug Fix
548, Duplicate Segments
549, Clone Coin Mechanism
550, Open Coinset File
551, Open Log File
560, Important:
561, Due to variations between coin validators, no guarantee is given
562, or implied as to the specific performance of mechanisms programmed
563, using this generic coinset. Please verify that the coin discrimination
564, after programming is satisfactory for your application
565, Click OK to proceed
566, Mektek Europe Ltd
600, Not a valid Credit Issue Message
601, Checksum error in the Credit Issue Message
602, Credit Issue Message is not for this Serial Number
603, Credits Loaded OK
604, Credit Load
605, Error
606, Not a valid Refund Permit Message
607, Checksum error in the Refund Permit Message
608, Refund Permit is not for this Serial Number
609, Send Message String to your VAR
610, Refund Complete
611, Error
612, Error loading Credits form form : 
613, Message Checksum Error
614, Message Not Accepted
615, Message Not Accepted
616, Incorrect VAR Code
617, Incorrect VAR Code
618, Incorrect Code
619, Error Decoding Received Credit data : 
620, Error Decoding Credit Request : 
621,  Expired
622, Error Decoding Audit message : 
623, Error Decoding Refund message : 
624, Error Deduct Authorised message : 
625, Validation Error
626, Error Writing Unit Config File : 
627, Error Writing Unit Transaction Log File : 
650, Unit Serial Number
651, Today's Date
652, Available
653, Used
654, Added
655, Refunded
656, Standard Credits
657, Available
658, Used
659, Expiry
660, Code String
661, Request More Credits
662, Number requested
663, Load New Credits
664, Number Loaded
665, Back to Main Window
666, Promotional Credits
700, Error Unloading EEPROM Data form : 
701, Invalid Filename
702, Error
703, Confirm overwrite EEPROM
704, Write EEPROM
705, Error Programming EEPROM routine : 
706, Error in Read EEPROM command : 
707, Error Refreshing the EEPROM display : 
708, Confirm overwrite EEPROM
709, Write EEPROM
710, Unable to deduct Credits
711, Credits
712, Invalid Routing Path entered
713, Error
714, Invalid Binary Code entered
715, Error
716, Error Programming Routing Data : 
717, Save File
718, Overwrite Existing File
719, Warning
720, Error Programming EEPROM routine : 
721, Error Loading EEPROM Data form : 
722, Hex Data 
723, Limits
724, Other Information
725, Error Initialising EEPROM display form : 
726, C450 Routing
727, Coin 
728, Route 
729, Sentinel Routing
730, Coin 
731, Route : 
732, C120 Output Mapping
733, Jaguar C120 Output
734, New C120 Output
735, No other Information available
736, Error Displaying EEPROM Data : 
750, DATA READ FROM EEPROM
751, C435 Ancilliary Settings
752, Path
753, 1st
754, 2nd
755, 3rd
756, 4th
757, Binary
758, Routing
759, Memory
760, Plug
761, Plug Default Route
762, Mech Type
763, Display
764, Read EEPROM
765, Save to File
766, Programme Routing
767, Programme from File
768, Close Window
800, Error loading Program CC Mech form : 
801, Error loading NRI Program Mech form : 
802, Error launching NRI Utility form : 
803, Error launching CC Utility form : 
804, Error launching Validator Test form : 
805, Error loading Program Mars Mech form : 
806, Error launching Validator Test form : 
807, Error launching PROM Utilities form : 
808, Error launching Validator Test form : 
809, Error in COM port reception routine : 
810, Mektek Programmer is already Running
811, Error
812, English
813, System date needs resetting
814, Error
815, Error loading Main form : 
816, Battery Low
817, Warning
818, Error Decoding Received data : 
819, Error Displaying Accepted Coin : 
820, Error Decoding Idle Values : 
821, Error Displaying G10 Accepted Coin : 
822, Error Displaying Sentinel Accepted Coin : 
823, Error Initialising the selected COM port : 
824, Windows has port COM
825,  open already
826, Error
827, Programmer Software is only compatible with Mars Coin Mechs
828, Contact Mektek or your VAR to upgrade
829, Warning
830, Error Decoding Timing Values : 
831, Error Counting down timer 1 : 
832, Error Writing Config Default File : 
833, Error Counting down timer 2 : 
834, Error Counting down timer 3 : 
835, Error Making Sound : 
850, Configuration
851, Select Serial Port
852, COM 1
853, COM 2
854, COM 3
855, COM 4
856, Language
857, Credits Warning Level
858, Save Config
859, Cancel
860, Program Mech
861, Validator Test
862, PROM Utilities
863, Program Mech
864, Validator Test
865, EEPROM Utilities
866, Program Mech
867, Validator Test
868, Memory Utilities
869, Program Mech
870, Validator Test
871, PROM Utilities
872, Exit
873, Load Credits
874, Change Config
875, Software Version Number
876, Programmer Version Number
900, Error Unloading EEPROM Data form : 
901, Unable to deduct Credits
902, Credits
903, Open File
904, Invalid Filename
905, Error
906, Confirm overwrite Memory
907, Write EEPROM
908, Memory Write
909, WRITING MEMORY IN PROGRESS
910, Data Written OK
911, OK
912, Error Writing Data
913, Error
914, Error Programming NRI Memory routine : 
915, Error in Read EEPROM command : 
916, Error Refreshing the Memory display : 
917, Save File
918, Overwrite Existing File
919, Warning
920, Error Programming NRI data file : 
921, Error Loading EEPROM Data form : 
922, Limits
923, Parameter Map
924, Compensation Map
925, Other Information
926, Error Initialising NRI memory display form : 
927, Coin 
928, Parameter 
929, NFP
930, GRO
931, GRU
932, NFA
933, RCH
934, HFP
935, Coin 
936, 00=hfp  01=nfa  02=gro  03=hfa  04=nfp  05=hxn  06=hxa  07=snp
937, 08=shp  09=m09  10=m10  11=m11  12=m12  13=m13  14=m14  15=m15
938, CP1H = 
939,    CP1L = 
940,    CP2H = 
941,    CP2L = 
942, Output Hex   Inhibit No      Value    Pulses
943, Coin 
944, Value Multiplier: 
945, Value
946, Coin 
947, Value
948, LMR
949, Map
950, Coin 
951, Lowest Value
952, Left Tube Value   
953, Mid Tube Value    
954, Right Tube Value  
955, Value
956, Coin 
957, Value Multiplier: 
958, Last Adjustment:  
959, Error Displaying EEPROM Data : 
970, DATA READ FROM NRI MEMORY
971, Mech Type
972, Display
973, Read Memory
974, Save to File
975, Programme from File
976, Close Window
977,    Route
1000, Checking for Communication with Mektek Programmer
1100, PROM PROGRAMMING IN PROGRESS
1101, Segment
1200, Error Unloading PROM form : 
1201, Error Changing PROM Limits : 
1202, Error Launching PROM Data form : 
1203, Limits edited - OK to use new values 
1204, CANCEL to abort programming
1205, Limits Changed
1206, Unable to deduct Credits
1207, Credits
1208, Insert 
1209,  Bipolar PROM
1210, Load PROM
1211, Bipolar PROM is not blank
1212, Press OK to programme anyway
1213, Press CANCEL to abort
1214, PROM
1215, Insert Mektek E+1 PROM : BOTH SWITCHES ON
1216, Load PROM
1217, Mektek E+1 PROM : TURN SWITCH 2 OFF
1218, Load PROM
1219, Error Programming PROM routine : 
1220, Error Restoring Limits : 
1221, Error Launching Validator Test : 
1222, Error Clearing Overlap Colours : 
1223, Error Calculating Overlap of Limits : 
1224, Error Calculating Acceptance / Rejection Rates : 
1225, Error Displaying Acceptance Rates : 
1226, Display PROM Segment
1227, Program New PROM
1228, PROM Utilities
1229, Coin 
1230, Display EEPROM Segment
1231, Program EEPROM
1232, EEPROM Utilities
1233, Coin 
1234, Error Initialising Limits Display form : 
1235, Limits edited - using new values 
1236, Limits Changed
1237, Coin 
1238, Coin 
1239, Error Selecting PROM Segments : 
1250, Limits
1251, Thickness
1252, Thickness
1253, Thickness
1254, Thickness
1255, Thickness
1256, Thickness
1257, Est Acceptance %
1258, Coin A
1259, Coin A
1260, Coin A
1261, Coin A
1262, Coin A
1263, Coin A
1264, Coin A
1265, Coin A
1266, Est. Rejection %
1267, Slug 1
1268, Slug 2
1269, Slug 3
1270, Slug 4
1271, Slug 5
1272, Slug 6
1273, Restore Limits
1274, Change Limits
1275, Display PROM segments
1276, PROM size
1277, Mech Type
1278, Target PROM Type
1279, Mektek E+1
1280, Bipolar
1281, Program New PROM
1282, Validator Test
1283, PROM Utilities
1284, Back to Measurement Window
1300, Error Selecting Mech Type for PROM : 
1301, Error Selecting PROM Size for display : 
1302, Error Unloading PROM Data form : 
1303, Error in Read PROM command : 
1304, Error Refreshing the PROM display : 
1305, Error Loading PROM Data form : 
1306, Data Addr 0-255
1307, Limits Segs 1 & 2
1308, Data Addr 256-511
1309, Limits Segs 3 & 4
1310, Data Addr 0-255
1311, Limits & Values
1312, Data Addr 256-511
1313, Error Building PROM display selection lists : 
1314, Error Initialising PROM display form : 
1350, DATA READ FROM PROM
1351, NEW PROM DATA TO PROGRAM
1352, Mech Type
1353, Display
1354, PROM size
1355, Read PROM
1356, Close Window
1400, Error Closing Validator Test form : 
1401, Error Opening Validator Test form : 
1402, Coin 
1403, Coin 
1404, Rejected
1405, Error setting up Validator Test form display : 
1406, Remove Programming Loom
1420, Coin Count
1421, Coin Count
1422, Mech Type
1423, Coin A
1424, Coin B
1425, Coin C
1426, Coin D
1427, Coin E
1428, Coin F
1429, Coin G
1430, Coin H
1431, Coin I
1432, Rejected
1433, Rejected
1434, Rejected
1435, Rejected
1436, Rejected
1437, Rejected
1438, Rejected
1439, Output Mode
1440, Single
1441, Binary
1442, Clear Counts
1443, Back to Main Menu
1444, Test Coin Mech
1445, Tube L
1446, Tube M
1447, Tube R
1448, Cashbox
